INSTALL COM PORT CONVERT DRIVER

Insert CA-232 to your laptop or PC, system will install the driver automatically. If the driver is required, then specify its path ¡§E:\USB DRIVER\CDM 2.08.24 WHQL Certified X86-32bit¡¨. (E: is your CD-ROM drive)


SOFTWARE INSTALLATIION

Insert the CD into your PC¡¦s CD-ROM drive. It should begin running the installation program, if you have auto-execute enabled.

When the installation screen was shown, click NEXT to install the software.

If you do not have auto-execute enabled for your PC¡¦s CD-ROM drive, navigate to the root directory of the CD using Windows Explorer and click on the file named Setup.exe. This will open the installation window. Then click NEXT to install the software.




