The following registry keys are an example of what would be required to have your device install 

without user interaction.

To obtain a more accurate set of registry settings first install your device then extract the registry

settings from your target using Embedded Visual C++ registry editor or similar. The settings that are relevant 

are in the HKEY_LOCAL_MACHINE\Drivers\USB section.



[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\FTDI_DEVICE]

"Prefix"="COM"

"Dll"="ftdi_ser.dll"

"ConfigData"=hex:\

      01,00,3f,3f,10,27,88,13,c4,09,e2,04,71,02,38,41,9c,80,4e,c0,34,00,1a,00,0d,\

      00,06,40,03,80,00,00,d0,80

"InitialIndex"=dword:00000000

"DeviceArrayIndex"=dword:00000000

"LatencyTimer"=dword:00000010



[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\1027_24577\Default\Default\FTDI_DEVICE]

"DLL"="ftdi_ser.dll"



[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\Default\Default\255\FTDI_DEVICE]

"DLL"="ftdi_ser.dll"

